WONGA OUTFALL

Click the photograph for a enlarged view

General Description

Sewerage Catchment:

- The Wonga Point outfall is the discharge point for the Bateau Bay STP.

Sewage Treatment:

- Bateau Bay uses a continuous extended aeration activated sludge (CEASS) process with trickling filters and disinfection by chlorination.

Outfall:

- The outfall was commissioned in 1971 and is located at Wonga Point. The discharge pipe is located at the edge of the rock platform below low tide.

Outfall Site

Wonga

(Wong_2) Last updated June 2000