BOAMBEE HEAD OUTFALL

Click the photograph for a enlarged view

Discharge Characteristics

Design Capacity: | Sewerage System | N/A
| STP
| N/A
| Outfall | N/A

Flows: | Average flow ~ 2.6 ML/day with typical discharge operations involve pumping for about 25 minutes at the rate of 360L/s on a 50 minute cycle, about 8 times a day

Effluent Quality: | CLICK here for recent data.

E PA Licence No:

Outfall Site

Boambee

(Boam_3) Last updated May 2000