STOCKTON OUTFALL

Click the photograph for a enlarged view

General Description

This outfall was constructed in 1936.

Sewerage Catchment:

- Stockton outfall is the discharge point for the Stockton STP.

Sewage Treatment:

- Stockton STP pr ovides secondary treatment effluent (Imhoff tank, oxidation ponds and surface aerators).

Outfall:

- Effluent is discharged into the surf zone on Stockton Beach via an elevated trestle pipeline located about 2km north of the entrance to Newcastle Harbour (MHL769 1997).

Outfall Site

Stockton

(Stoc_2) Last updated May 2000