CAMDEN HAVEN OUTFALL

Click the photograph for a enlarged view

General Description

Camden Head outfall is the discharge point for the Camden Haven STP.

Sew er age Catchment:

- Camden Haven STP uses a secondary treatment process together with trickling filters and disinfection by chlorination (MHL769 1997).

Sewage Treatment:

- Camden Haven STP uses a secondary treatment process together with trickling filters and disinfection by chlorination (MHL769 1997).

Outfall:

- The ocean outfall is located on the southern side of Camden Head approximately 1km south of the Camden Haven River entrance. A 600mm diameter pipe discharges at the shoreline through placed boulders (see photo).

Outfall Site

Camden Haven

(Camd_2) Last updated May 2000