RED POINT OUTFALL

Click the photograph for a enlarged view

Discharge Characteristics

Design Capacity: | Sewerage System | N/A
| STP |
| Outfall | N/A

Flows: | Average dry weather flow ~ 16.1 ML/day (MHL769 1997).

Effluent Quality: | CLICK here for recent data.
| See also Patterson, Britton & Partners, CEE & AWT (1998).

E PA Licence No:

Outfall Site

Red Point

(Redp_3) Last updated June 2000