PENGUIN HEAD OUTFALL

Click the photograph for a enlarged view

Discharge Characteristics

Design Capacity: | Sewerage System | N/A
| STP |
| Outfall | N/A

Flows: | Effluent is released ~ 90 L/s for a duration of 3 to 5 hours per day. Annual effluent volume ~ 500 ML (average 2ML/day - MHL769 1997). Existing and projected effluent flow rates and effluent quality are included in Tables 1.2 to 1.5.

Effluent Quality: | CLICK here for recent data.
| See also MHL746 1996, Patterson, Britton & Partners 1995 and EPA licence compliance reports).

E PA Licence No:

Outfall Site

Penguin Head

(Peng_3) Last updated June 2000