CORAMBIRRA OUTFALL

Click the photograph for a enlarged view

Discharge Characteristics

Design Capacity: | Sewerage System | N/A
| STP | N/A
| Outfall | N/A

Flows: | Average flow ~ 6.6 ML/day, pump capacity is 780 L/s and reclaimed water is discharged intermittently approximately 3 minutes every 20 minutes

Effluent Quality: | CLICK here for recent data.

E PA Licence No: |

Outfall Site

Corambirra

(Cora_3) Last updated May 2000