THE LADDERS OUTFALL

Click the photograph for a enlarged view

Discharge Characteristics

Design Capacity: | Sewerage System | N/A
| STP | 15,000 EP
| Outfall | N/A

Flows: | Average dry weather flow ~ 36 L/s (min. ~ 18L/s and max. ~ 65 L/s). This equates to approximately 3.6 ML/day.

Effluent Quality: | CLICK here for recent data.
| See also MHL516 1988

E PA Licence No:

Outfall Site

The Ladders

(Ladd_3) Last updated June 2000