BOMBO OUTFALL

Click the photograph for a enlarged view

Discharge Characteristics

Design Capacity: | Sewerage System | N/A
| STP | 9,500 EP
| Outfall | N/A

Flows: | Average flow ~ 2.7 ML/day (MHL769 1997); current wet weather flows up to 38.8 ML/day could receive full secondary treatment (wet weather flows up to 28 ML/day currently receive full secondary treatment and disinfection with the rest only partially treated before being recombined with the fully treated effluent before disinfection and discharge through the ocean outfall.

Effluent Quality: | CLICK here for recent data.
| See also Sydney Water Corporation (1998k)

E PA Licence No:

Outfall Tunnel

Bombo

(Bomb_3) Last updated June 2000