FORSTER OUTFALL

Click the photograph for a enlarged view

Discharge Characteristics

Design Capacity: | Sewerage System | N/A
| STP | 13,200 EP at present (32,400 EP by the year 2016)
| Outfall | N/A

Flows: | Average flow ~ 3.6 ML/day (Manidis Roberts 1993) discharged at approximately 200L/s for up to five hours each night under normal dry weather conditions.

Effluent Quality: | CLICK here for recent data.
| See also (MHL640 1993)

E PA Licence No:

Outfall Site

Forster

(Fost_3) Last updated May 2000