BELLAMBI OUTFALL

Click the photograph for a enlarged view

Discharge Characteristics

Design Capacity: | Sewerage System | N/A
| STP |
| Outfall | N/A

Flows: | Average dry weather flow ~ 20 ML/day (MHL769 1997).

Effluent Quality: | CLICK here for recent data.
|

E PA Licence No: | See also Patterson, Britton & Partners, CEE & AWT 1998 & Sydney Water Corporation 1998g.

Outfall Site

Bellambi

(Bell_3) Last updated June 2000