SYDNEY'S DEEP OCEAN OUTFALL

Click the photograph for a enlarged view

Discharge Characteristics

Design Capacity: | Sewerage System | N/A
| STP |
| Outfall | N/A

Flows: | North Head average flow ~ 293 ML/day.
| Bondi average flow ~ 141 ML/day.
| Malabar average flow ~ 475 ML/day.

Effluent Quality: | CLICK North Head, Bondi or Malabar for recent data.
|

E PA Licence No:

Sydney's Deep Ocean Outfalls

(Deep3_3) Last updated June 2000