NORAH HEAD OUTFALL

Click the photograph for a enlarged view

General Description

Sewerage Catchment:

- Norah Head outfall discharges the combined effluents from Mannering Park, Wyong South, Gwandalan, Toukley and Charmhaven STPs.

Sewage Treatment:

- Toukley STP uses trickling filters. The other four STPs use the IEEAS process and

Outfall:

- The outfall was commissioned in 1988 and is located at Norah Head. It has three stainless steel nozzles, each with a diameter of 280mm located approximately 4 meters below mean sea level.

Outfall Site

Norah Head

(Nora_2) Last updated June 2000