BURWOOD BEACH OUTFALL

Click the photograph for a enlarged view

Discharge Characteristics

Design Capacity: | Sewerage System | N/A
| STP |
| Outfall | N/A

Flows: | Average flow ~ 40 ML/day of effluent and 2 ML/day of sludge. Effluent flow rates range from about 450 L/s up to 5900 L/s in peak wet weather conditions. Sludge pumped at a rate of 25 to 30 L/s is mixed with effluent and pumped at a rate of 15 to 20 L/s to produce a “shandy” discharge of 40 to 45 L/s in addition to the effluent discharge.

Effluent Quality: | CLICK here for recent data.
| See also HWC 1992 and Laxton & Laxton 1989

E PA Licence No:

STP Location

Burwood Beach

(Burw_3) Last updated May 2000