TURIMETTA HEAD OUTFALL

Click the photograph for a enlarged view

Discharge Characteristics

Design Capacity: | Sewerage System | N/A
| STP | 61,900EP
| Outfall | N/A

Flows: | Average dry weather flow ~16 ML/day; maximum dry weather flow ~ 35.2 ML/day and maximum wet weather flow ~ 115 ML/day (Sydney Water Corporation 199b).

Effluent Quality: | CLICK here for recent data.

E PA Licence No: |

Outfall Site

Turrimetta Head

(Turi_3) Last updated May 2000