ULLADULLA OUTFALL

Click the photograph for a enlarged view

General Description

Sewerage Catchment:

- Ulladulla outfall is the discharge point for the Milton/Ulladulla STP, which services the communities of Ulladulla and Milton.

Sewage Treatment:

- The Milton/Ulladulla STP uses a CEAAS treatment process with trickling filters, but no tertiary treatment. Disinfection of effluent is currently undertaken during the summer months.

Outfall:

- The outfall consists of a 600mm pipe and is located on the rock platform at Warden Head.

Outfall Site

Ulladulla

(Ulla_2) Last updated June 2000