POTTER POINT OUTFALL

Click the photograph for a enlarged view

Future Developments

An upgrade of the treatment process at Cronulla STP is currently being undertaken and is planned for completion in the year 2000. The upgraded STP will include:

- secondary and tertiary treatment for flows up to 171 ML/day;

- primary treatment for flows up to 432 ML/day;

- fine screening for flows up to 432 ML/day;

- disinfection (UV) of all flows.

- Connection of Bundeena and Mainbar to existing system (Sydney Water Corporation 1998f).

Potter Pt.

(Pott_4) Last updated June 2000