CONISTON BEACH OUTFALL

Click the photograph for a enlarged view

Discharge Characteristics

Design Capacity: | Sewerage System | N/A
| STP | 61,900EP
| Outfall | N/A

Flows: | Average dry weather flow ~ 13.2 ML/day (MHL769 1997).

Effluent Quality: | CLICK here for recent data.
| See also Patterson, Britton & Partners, CEE & AWT

E PA Licence No:

Diffuser Head

Coniston Beach

(Coni_3) Last updated May 2000