SKENNARS HEAD OUTFALL

Click the photograph for a enlarged view

Discharge Characteristics

Design Capacity: | Sewerage System | N/A
| STP | 58000EP (?)
| Outfall | N/A

Flows: | Highly variable from 1.7ML/d (dry, off peak) to 6ML/d (wet weather)
| Daily dry loads from ~1.95ML to ~ 2.2ML (median 2.09ML)
| Daily wet weather loads (20 to 30 mm of rainfall – i.e. mild event) ~ 3ML/d

Effluent Quality: | CLICK here for recent data.
| See also Camp, Scott & Furphy (1990).

E PA Licence No:

Outfall Site

Skennars Head

(Sken_3) Last updated May 2000