PLANTATION POINT OUTFALL

Click the photograph for a enlarged view

General Description

Sewerage Catchment:

- Plantation Point outfall is the discharge point for effluent from Huskisson and St Georges Basin STPs

Sewage Treatment:

- Huskisson STP is an activated sludge plant with tertiary ponding. St Georges Basin STP is also an activated sludge plant with tertiary ponding, phosphorus removal

Outfall:

- The outfall is located at the end of Plantation (=Lamb’s) Point, east of the township of Vincentia and within the confines of Jervis Bay. The outfall discharges at the edge of a rock platform into water depths of approximately 2 m.

Outfall Site

Plantation Pt.

(Plan_2) Last updated June 2000